

 **Model: BC-DTS150-10**

**150W DC-10GHz RF Attenuator**

Coaxial fixed attenuators are used in absorbing energy of transmission line, expanding power range and controlling power level, they are also used in accurately measuring power or spectrum of RF microwave transmitters accompany with small power meter, comprehensive tester or spectrum analyzer.

|  |  |
| --- | --- |
| **Technical Data Sheet** | |
| Frequency Range | DC~10GHz |
| Connectors | N,7/16 (DC-4GHz) |
| Body Material and Plating | Aluminum, Black Anodize |
| Power | 150W |
| Peak Power | 5KW ((5μs pulse width, 3% duty circle ) |
| Impedance | 50Ω |
| Temperature Range | -55°C～+125°C |
| Dimensions | A:173×130×75mm; B:173×78×78mm; E2: 85×86×173mm |
| Weight | A:1.5Kg; B:1.5Kg; E2:1.5Kg |





Tolerance：±5%